Maintenance

# Cleaning the Scanner

> Cleaning the internal glass

To keep your scanner operating at its best, clean it periodically, as follows:

| Turn off the scanner, and then unplug the power cord.

| Clean the outer case of the scanner and the source holders with a cloth dampened with mild detergent and water.

| Caution:

Never use alcohol, thinner, or corrosive solvent to clean the scanner. These chemicals can damage the scanner components as well as the case.

Be careful not to spill liquid into the scanner mechanism or electronic components. This could permanently damage the mechanism and circuitry.

Do not spray lubricants inside the scanner.

Never open the scanner case.

## Cleaning the internal glass

If you can find that a printed image contains unexpected lines, clean the internal glass with a cleaner.

| Turn off the scanner, and then unplug the power cord.

| Insert the cleaner in the holder slot.

|  | Note:

You can use both side of the cleaner.

| When the cleaner reaches a certain position, eject the cleaner. Using the cleaner to clean the internal glass once is enough.

|  | Note:

After using the cleaner, keep the cleaner in a bag to prevent dust and moisture.

[Top]

Next