Product Information / Technical Specifications

# Scanning

Scanner type | Color
Photoelectric device | Color CCD line sensor
Effective pixels | 12800 x 31622 pixels at 3200 dpi, 100% Reflective: 12848 x 19280 pixes at 3200 dpi, 100%l Transparency: 13232 x 28976 pixels at 3200 dpi, 100%
Document | 35 mm strip film 35 mm slide Medium format (120/220): max 6 x 18 cm (eg. 6 x 9 cm (2 frames)) strip films 4 x 5 inch film Reflective documents in up to 4 x 6 inch in size
Scanning resolution | 3200 dpi (main scan) 6400 dpi with Micro Step (sub scan)
Output resolution | 50 to 6400 dpi (50 to 6400 dpi in 1 dpi increments, 12800 dpi. 12800 dpi performed with zoom function)
Color separation | RGB color filters on CCD
Image data | 16 bits per pixel per color internal 16 bits per pixel per color external
Color correction | 2 type for user-defined
Interface | USB 2.0 (Type B Receptacle Connector), USB 1.1 (Type A Receptacle Connector), and IEEE 1394 Serial Bus Interface
Light source | White cold cathode fluorescent lamp

[Top]

Previous | Next