Maintenance

# Replacing the Fluorescent Lamp

The luminosity of the fluorescent lamp declines over time. If the lamp breaks or becomes too dim to operate normally, the scanner stops working and E rror lights on. When this happens, the lamp assembly must be replaced. For details, contact your dealer.

| Caution:

Never open the case of the scanner. If you think repairs or adjustments are necessary, consult your dealer.

[Top]

Previous | Next