Product Information

# Scanner Parts

> Front
> Back
> Lights
> Buttons and slots

## Front

> 1. Setup button
> 2. Scan&Memory button
> 3. Professional Lab button
> 4. Photo Print button
> 5. Card access light
> 6. Memory card slots
> 7. Power button
> 8. Error light
> 9. Holder slot
> 10. Allow buttons
> 11. Start button
> 12. Transmitting light
> 13. OK button
> 14. Eject button
> 15. Cancel button

[Top]

## Back

> 1. DC inlet
> 2. IEEE1394 cable connector
> 3. USB cable connector for printer
> 4. USB cable connector for computer

[Top]

## Lights

Lights | Color | Indicator Status | Function
Transmitting | Blue | Single Flashing | Single flashes when the scanner is turned on.
3 Flashing | 3 flashes when the scanner connects to a USB host.
Flashing | Flashes when the scanning operation is in progress, or when the scanner is transmitting data to a printer or a memory card.
Error | Red | On | Indicates a variety of error conditions. For detail see Error Indicator.
OFF
Memory card access light | Green | On | Light up when a memory card is inserted or not accessed, and flashes when the memory card is being accessed. It turns off when the memory card is not loaded.
Flashing
Off

[Top]

## Buttons and slots

Button/slot | Function
Power | Turns the scanner on and off.
Start | Starts scanning, printing and saving to memory card.
OK button | Decides an image to print. Saves a setting change.
Photo Print button | Makes prints. Pressing this button displays a screen for selecting a document. During the Photo Print operation, this button lights up.
Professional Lab button | Trims or retouches scanned images. Pressing this button displays a screen for selecting a document. During the Professional Lab operation, this button lights up.
Scan& Memory button | Saves a scanned image to a memory card. During the Scan& Memory operation, this button lights up.
Setup button | Starts the maintenance of the scanner and printer, deletes images from a memory card, or selects a language. Pressing this button displays the Setup function menu. During the setup operation, this button lights up.
Allow buttons | Select menu items. Adjust the frame for trimming a scanned image. The light on the center of these buttons flashes, while the scanner is transmitting a scanned image to your computer or printing an image.
Cancel button | Clears the settings you have entered. Resets the values of settings, and stops operations.
Eject button | Ejects a source holder from the holder slot.
Memory card slots | Insert a memory card in the slot specified for the type of the card.
Holder slot | Insert a source holder with films or documents here.

[Top]

Previous | Next