WALKMAN User Guide
Print
Top page > How to Use the Speaker > Parts and Controls of the Speaker > Installation (NWZ-E463K/E464K only)

## Installation (NWZ-E463K/E464K only)

Notes on installation
Installing the stand
Note

- Do not place the speaker in an inclined position.

- Do not place the speaker in locations that are hot or subject to direct sunlight, dust, high humidity, or extreme cold.

- Use caution when placing the speaker on a specially treated (waxed, oiled, polished, etc.) floor, as staining or discoloration may result.

1. Set up the stand located on the rear side of the speaker ().

1. Install your “WALKMAN” in the speaker.

### Notes on installation

- When a strap is attached to your “WALKMAN,” set it under and out to the front of your “WALKMAN.” Before using the speaker, check that the strings of the strap are not in the curved groove.

- At purchase, the attachment for your “WALKMAN” is set into the speaker. If the attachment becomes detached, slide and set it into the speaker until it clicks as shown in the illustration.

### Installing the stand

When the stand becomes detached, install the stand into the speaker by following the procedure below.

1. Be sure to fit the upper right hinge of the stand on the right side pin on the rear of the speaker first.

1. Hinge

1. Right side pin

1. Fit the other hinge on the left pin, and then press down the stand until it clicks.

Go to page top