Product Information / Technical Specifications

# System Requirements and Compatibility

> For Windows PCs
> For Macintosh

Refer to the appropriate section below for the minimum and recommended computer system requirements necessary to use scanner software.

## For Windows PCs

### For USB 1.1 users

System | Microsoft® Windows® XP, Me, Windows 98, or Windows 2000 preinstalled
Interface | Computer's USB port (TYPE A receptacle)
Display | SVGA or higher resolution monitor 800 x 600 screen resolution or higher and 16 bits (High Color) Note: Color and tone reproduction are subject to the display capability of your computer system, including the video card, display monitor, and software. See the product documentation for details.

### For USB 2.0 users

System | Microsoft® Windows® XP or Windows 2000 preinstalled
Interface | Computer's USB port (TYPE A receptacle)
Display | SVGA or higher resolution monitor 800 x 600 screen resolution or higher and 16 bits (High Color) Note: Color and tone reproduction are subject to the display capability of your computer system, including the video card, display monitor, and software. See the product documentation for details.

### For IEEE 1394 users

System | Microsoft Windows XP, Me, or Windows 2000 Note: Windows 98 is not supported.
Interface | IEEE 1394a-2000 compatible
Display | SVGA or higher resolution monitor 800 x 600 screen resolution or higher and 16 bits (High Color) Note: Color and tone reproduction are subject to the display capability of your computer system, including the video card, display monitor, and software. See the product documentation for details.

[Top]

## For Macintosh

### For USB 1.1 users

System | Mac OS® 8.6, 9.0 to 9.2, Mac OS X 10.2 or later Note For Mac OS X 10.3 users: Fast User Switching is not supported.
Interface | Macintosh USB
Display | Color monitor, 800 x 600 screen resolution (or higher recommended), and 32,000 colors (or higher) Note: Color and tone reproduction are subject to the display capability of your computer system, including the video card, display monitor, and software. See the product documentation for details.

### For USB 2.0 users

System | Mac OS® X 10.2.7 or later Note For Mac OS X 10.3 users: Fast User Switching is not supported.
Interface | Macintosh USB
Display | Color monitor, 800 x 600 screen resolution (or higher recommended), and 32,000 colors (or higher) Note: Color and tone reproduction are subject to the display capability of your computer system, including the video card, display monitor, and software. See the product documentation for details.

### For FireWire users

System | Mac OS® 8.6, 9.0 to 9.2, Mac OS X 10.2 or later Note For Mac OS X 10.3 users: Fast User Switching is not supported.
Interface | IEEE 1394a-2000 compatible
Display | Color monitor, 800 x 600 screen resolution (or higher recommended), and 32,000 colors (or higher) Note: Color and tone reproduction are subject to the display capability of your computer system, including the video card, display monitor, and software. See the product documentation for details. Make sure FireWire 2.1 or later is installed on your computer. Download FireWire's update file from the website of Apple Computer, Inc, and then install it on your computer.

[Top]

Previous | Next